How to get genesis xband modem working......


Do modification to hardware
flash master or slave rom (with debugger program integrated into rom) to xband modem depending on what you want to be.

then control the modem with the program in dev_c.zip

send the game patch to the sram

launch the game. 

both modems must be connected together via direct phone cord.

here is where serial to rj45 comes in. make adaptor that will allow you to 
send the data over to a computer serial port then over tcp/ip to another pc which then transfers it back into serial and then into the xband..

This should be ok to work

OR eliminate serial to rj45 and go with serial to ethernet adaptor
use a pic ethernet adaptor that can be programmed on the fly for what ip address to connect to.


